## SRS

#### General Troubleshooting Information (cont'd)

23-37

- Including the most recent problem, up to three different malfunctions can be indicated (see example 1 below).
- In case of a continuous failure, the DTC will be indicated repeatedly (see example 1 below).
- In case of an intermittent failure, the SRS indicator light will indicate the DTC one time, then it will stay on (see example 2 below).
- If both a continuous and an intermittent failure occur, both DTCs will be indicated as continuous failures.
- When the system is normal (no DTC), the SRS indicator light will stay on (see example 3).
- If the SRS indicator light comes on continuously without a DTC, there may be a problem with the system.
- If the SRS indicator light does not come on as indicated above, always check for an open or a short to ground in the SCS circuit before troubleshooting the system.

Example of the DTC Indications: