## Manual Transmission

#### Transmission Removal (cont'd)

13-8

24. Remove the engine stiffener (A) and clutch cover (B).

Steel oil pan type:

Aluminium oil pan type:

25. Place the transmission jack under the transmission and remove the three lower transmission mounting bolts.

26. Pull the transmission away from the engine until the transmission mainshaft clears the clutch pressure plate, then lower the transmission on the transmission jack.
27. Remove the boot (A), the release fork (B) and the release bearing (C) from the transmission (D).