## Honda Multi Matic Transmission/CVT

#### DTC Troubleshooting (cont'd)

14-292

DTC 6: Open in Transmission Range Switch Circuit

1. Test the transmission range switch (see page 14-350).

Is the switch OK?

YES - Go to step 2.

NO - Replace the transmission range switch.

2. Connect the transmission range switch connector.
3. Check for continuity between PCM connector terminal A23 and body ground and between terminal A24 and body ground.

PCM CONNECTOR A (31P)

Wire side of female terminals

Is there continuity?

YES - Go to step 4.

NO - Repair open in the wires between PCM connector terminals A23 and A24 and ground (G101), or repair poor ground (G101).

4. Turn the ignition switch ON (II).

5. Shift to position.

6. Measure the voltage between PCM connector terminals C20 and A23 or A24.

PCM CONNECTORS

Wire side of female terminals

Is there voltage?

YES - Repair open in the wire between PCM connector terminal C20 and the transmission range switch.

NO - Go to step 7.

7. Shift to position.
8. Measure the voltage between PCM connector terminals C10 and A23 or A24.

PCM CONNECTORS

Wire side of female terminals

Is there voltage?

YES - Repair open in the wire between PCM connector terminal C21 and the transmission range switch.

NO - Go to step 9.