## Seats

#### Rear Seat Removal/Installation

20-40

NOTE: Take care not to scratch the body or tear the seat covers.

Remove the rear seat as shown. To remove the seat-back, remove the front portion of the trunk floor mat (see page 20-31).

Install the seat in the reverse order of removal, and note these items:

- Before installing the centre anchor bolts on the seat-back with the centre shoulder belt, make sure there are no twists or kinks in the belt.
- Make sure the seat-backs lock securely.

Fastener Locations

A : Bolt, 2 B : Bolt, 1 C : Bolt, 1 D : Clip, 2

1. PIVOT BUSHING
2. CENTRE BELT

   (For some models)

3. RIGHT SEAT-BACK
4. CENTRE PIVOT BOLT

   8 x 1.25 mm

   22 Nm (2.2 kgf/m, 16 lbf/ft)

5. 8 x 1.25 mm

   22 Nm (2.2 kgf/m, 16 lbf/ft)

6. HINGE COVER
7. SEAT-BACK CENTRE HINGE
8. BUSHING
9. LEFT SEAT-BACK
10. HOOK
11. CLIP
12. PIVOT BUSHING
13. 6 x 1.0 mm

    9.8 Nm (1.0 kgf/m, 7.2 lbf/ft)

14. SLITS
15. HOOK
16. SEAT CUSHION
17. SEAT BELT BUCKLE
18. CLIP
19. CENTRE ANCHOR BOLT

    7/16-20 UNF

    32 Nm (3.3 kgf/m, 24 lbf/ft)

a a a