## Design Specifications

####

2-12

Item | Measurement | Qualification | Specification
STARTER | Type |  | Gear reduction
Normal output |  | 1.1 kW
Hour rating |  | 30 seconds
Direction of rotation |  | Clockwise as viewed from gear end
CLUTCH | Clutch |  | Single plate dry, diaphragm spring
Clutch friction material surface area |  | 174 cm2 (26.97 sq in.)
MANUAL TRANSMISSION | Type |  | Synchronised, 6-speed forward, 1 reverse
Primary reduction |  | Direct 1:1
Gear ratio | 1st | 3.266
2nd | 2.130
3rd | 1.517
4th | 1.147
5th | 0.921
6th | 0.738
Reverse | 3.583
Final reduction | Type | Single helical gear
Gear ratio | 4.764
STEERING | Type |  | Rack and pinion, with electrical power assistance
Overall ratio |  | 14.49
Turns, lock-to-lock |  | 2.83
Steering wheel diameter |  | 380 mm (15.0 in.)
SUSPENSION | Type | Front | Strut
Rear | Double wishbone
Shock absorber | Front and rear | Telescopic, hydraulic, nitrogen gas-filled
WHEEL ALIGNMENT | Camber | Front | 0°
Rear | - 0°45'
Caster | Front | 1°33'
Total toe | Front | 0 mm (0 in.)
Rear | In 2 mm (1/16 in.)
BRAKES | Type of service brake | Front | Power-assisted self-adjusting ventilated disc
Rear | Power-assisted self-adjusting solid disc
Type of parking brake |  | Mechanical actuating, rear wheels
Pad friction surface area | Front | 49 cm2 x 2 (7.6 sq in. x 2)
Rear | 28 cm2 x 2 (4.3 sq in. x 2)
TYRES | Size of front and rear |  | 205/45R17 84W
Size of spare |  | T135/70D15 99M

a a a