## Cylinder Head

#### Valves, Springs and Valve Stem Seals Removal

6-21

Special Tools Required

- Remover/Installer valve guide 5-8840-9041-0
- Adapter valve spring 5-8840-7003-0

1. Remove the shim (A) and tappet (B).

   Be sure to keep the tappet and shim in order to reassemble in the original position.

1. Remove the split collar and valve spring using special tool (5-8840-7003-0).

1. Remove valves.

1. Be sure to keep the valve in order to reassemble in the original position.

1. Remove the valve stem seal.

a a a