## Hood

#### Adjustment

20-245

1. Slightly loosen each hood hinge bolt.
2. Adjust the hood alignment in this sequence.

- Adjust the hood right and left, as well as forward and rearward, by using the elongated holes on the hood hinge(A).
- Turn the hood edge cushions (B), as necessary, to make the hood fit flush with the body at the front and side edges.
- Adjust the hood latch (C) to obtain the proper height at the forward edge and move the hood latch right or left until the striker (D) is centred in the hood latch.

3. Tighten each bolt securely.