## Engine Assembly

#### Engine Removal (cont'd)

5-6

1. Disconnect the compressor clutch connector (A), then remove the harness clamp (B) and A/C compressor mounting bolts (C).

1. Remove the A/C compressor bracket, then remove the A/C compressor without disconnecting the A/C hoses.

1. Remove the water inlet hose (A), water outlet hose (B), expansion tank hose (C) and water hose (D).

1. Remove the upper radiator hose (A) and lower radiator hose (B).

a a a