## Engine Block

#### Crankshaft and Piston Removal

7-13

1. Remove the engine assembly (see page 5-3).

1. Remove the transmission (see page 13-5).

1. Remove the oil pan (see page 7-12).

1. Remove the oil pump (see page 8-11).

1. Remove the cylinder head (see page 6-25).

1. Remove the baffle plate.

1. Remove the 8 mm bolts.

1. Remove the bearing cap bolts. To prevent warpage, unscrew the bolts in sequence 1/3 turn at a time: repeat the sequence until all bolts are loosened.

1. Remove the lower block and bearings. Keep all bearings in order.

a a a