## Side Sill Outer Panel

#### Removal

3-52

- Cut and pry off the side sill outer panel.
- Check the centre pillar stiffener and side sill reinforcement position and for damage and if necessary, replace them.
- When removing the center pillar stiffener, do not cut the centre stiffener reinforcement; the centre pillar stiffener reinforcements is part of the centre pillar stiffener.
- When replacing the centre pillar stiffener, remove the centre pillar separator and glue the insulator at the separator mounted position.

  1. Outer panel cut line.
  2. Centre pillar stiffener cut line.
  3. CENTRE INNER PILLAR
  4. SIDE SILL REINFORCEMENT
  5. VIEW (Z)
  6. INSIDE SILL
  7. CENTRE PILLAR STIFFENER
  8. CENTRE PILLAR SEPARATOR
  9. SIDE SILL REINFORCEMENT
  10. OUTER PANEL
  11. CENTRE PILLAR STIFFENER REINFORCEMENT