## Clutch

#### Clutch Replacement (cont'd)

12-14

Flywheel Replacement NOTE: Do not disassemble the flexible plate.

1. Install the special tool.

2. Remove the flywheel mounting bolts in a criss-cross pattern in several steps, then remove the flywheel.

3. Remove the pilot bearing (A) from the flywheel (B).

4. Drive the new bearing into the flywheel using the special tools as shown. Apply a light coat of oil to the bearing surface.

5. Align the hole in the flywheel with the crankshaft dowel pin and install the flywheel. Install the washer and mounting bolts finger-tight.

6. Install the special tool, then torque the flywheel mounting bolts in a criss-cross pattern in several steps.