## Fuel Supply System

#### Fuel Pressure Relieving (cont'd)

11-116

Fuel Pressure Test

1. Disconnect the quick-connect fitting (A): Hold the connector (B) with one hand and squeeze the retainer tabs (C) with the other hand to release them from the locking pawls (D). Pull the connector off.

   NOTE:

- Prevent the remaining fuel in the fuel feed pipe or hose from flowing out with a rag or shop towel.
- Be careful not to damage the pipe (E) or other parts.
- Do not use tools.
- If the connector does not move, keep the retainer tabs pressed down, and alternately pull and push the connector until it comes off easily.
- Do not remove the retainer from the pipe; once removed, the retainer must be replaced with a new one.

1. After disconnecting the quick-connect fitting, check it for dirt or damage (see step 4 on page 11-120).

Special Tools Required

- Fuel pressure gauge, 07406-0040002
- Fuel pressure gauge set, 07ZAJ-S5A0100

1. Relieve the fuel pressure (see page 11-115).

1. Disconnect the quick-connect fitting (A). Attach the fuel pressure gauge set and fuel pressure gauge.

1. Start the engine and let it idle.

- If the engine starts, go to step 5.
- If the engine does not start, go to step 4.

1. Check to see if the fuel pump is running: listen to the fuel fill port with the fuel fill cap removed. The fuel pump should run for 2 seconds when the ignition switch is first turned on.

- If the pump runs, step 5.
- If the pump does not run, perform the fuel pump circuit troubleshooting, refer to the 2001 Civic Shop Manual (see page 11-112).

1. Read the pressure gauge. The pressure should be 320 - 370 kPa (3.3 - 3.8 kgf/cm2, 47 - 54 psi)

- If the pressure is OK, the test is complete.
- If the pressure is out of specification, replace the fuel pressure regulator and the fuel filter, refer to the 2001 Civic Shop Manual (see page 11-138), and recheck the fuel pressure.

a a a