## Air Conditioning

#### A/C Refrigerant Oil Replacement

21-67

NOTE: LHD type is shown, RHD type is similar.

1. CONDENSER
2. SUCTION LINE
3. HEATER UNIT
4. RECEIVER LINE B
5. SUCTION HOSE
6. RECEIVER LINE A
7. RECEIVER/DRYER
8. CONDENSER LINE
9. DISCHARGE HOSE
10. COMPRESSOR
11. COMPRESSOR BRACKET

1. Discharge hose to the compressor (6 x 10 mm) : 9.8 N m (1.0 kgf/m, 7.2 lbf/ft)
2. Discharge hose to the condenser (6 x 10 mm) : 9.8 N m (1.0 kgf/m, 7.2 lbf/ft)
3. Condenser line to the condenser (6 x 10 mm) : 9.8 N m (1.0 kgf/m, 7.2 lbf/ft)
4. Condenser line to the receiver/dryer (6 x 10 mm) : 9.8 N m (1.0 kgf/m, 7.2 lbf/ft)
5. Receiver line A to the receiver/dryer (6 x 10 mm) : 9.8 N m (1.0 kgf/m, 7.2 lbf/ft)
6. Receiver line A to the receiver line B : 13 N m (1.3 kgf/m, 9.4 lbf/ft)
7. Receiver line B and the suction hose to the evaporator (6 x 10 mm) : 9.8 N m (1.0 kgf/m, 7.2 lbf/ft)
8. Suction line to the suction hose : 31 N m (3.2 kgf/m, 23 lbf/ft)
9. Suction line to the compressor (6 x 10 mm) : 9.8 N m (1.0 kgf/m, 7.2 lbf/ft)
10. Compressor to the compressor bracket (8 x 1.25 mm) : 22 N m (2.2 kgf/m, 16 lbf/ft)
11. Compressor bracket to the engine block (10 x 1.25 mm) : 22 N m (4.5 kgf/m, 33 lbf/ft)