## Engine Assembly

#### Engine Removal (cont'd)

5-6

28. Disconnect the Primary Heated Oxygen Sensor (primary HO2S) connector (A) and Secondary Heated Oxygen Sensor (secondary HO2S) connector (B), then remove the exhaust pipe A/Three Way Catalytic Converter (TWC) (C) (Except D17A5 engine).

29. Remove the shift cable covers (A), then remove the shift control cable (B) (A/T).

30. Disconnect the suspension lower arm ball joints and stabiliser links, refer to the '01 Civic Shop Manual on this CD (see page 18-32).
31. Remove the driveshafts, refer to the '01 Civic Shop Manual on this CD (see page 16-3). Coat all precision finished surfaces with clean engine oil. Tie plastic bags over the driveshaft ends.

32. Lower the hoist.

33. Remove the ground cable (A), upper radiator hose (B), lower radiator hose (C) and heater hose (D).

34. Remove the heater hose.