## Driveline/Axle

#### Driveshafts Reassembly (cont'd)

16-15

1. Adjust the length of the driveshafts to the figure below, then adjust the boots to halfway between full compression and full extension. Make sure the ends of the boots seat in the grooves of the driveshaft and joint.

   Left driveshaft:

502 - 507 mm (19.8 - 20.0 in.)

Right driveshaft:

481 - 486 mm (18.9 - 19.1 in.)

1. Position the dynamic damper as shown below.

   Left driveshaft:

296 - 300 mm (11.7 - 11.8 in.)

1. Fit the boot (A) ends onto the driveshaft (B) and outboard joint (C).

a a a