## SRS

#### DTC Troubleshooting - with Side Airbags (cont'd)

23-120

5. Disconnect the IDi connector (A) from the driver's side impact sensor (B).

6. Disconnect the U2o connector (A) from the SRS unit (B).

7. Check resistance between the No. 8 terminal of the U2o connector and body ground. There should be 1 M ohm or more.

U2o CONNECTOR

Wire side of female terminals

Is the resistance as specified?

YES - Go to step 8.

NO - Short to ground in the floor wire harness; replace the floor wire harness.

8. Check resistance between the No. 8 and No. 15 terminals of the U2o connector. There should be 1 M ohm or more.

U2o CONNECTOR

Wire side of female terminals

Is the resistance as specified?

YES - Faulty driver's side impact sensor or SRS unit; replace the driver's side impact sensor. If the problem is still present, replace the SRS unit.

NO - Short in the floor wire harness; replace the floor wire harness.