## Honda Multi Matic Transmission/CVT

#### System Description (cont'd)

14-270

Electronic Control System (cont'd)

PCM Inputs and Outputs

PCM Connector Terminal Location

PCM CONNECTOR B (24P)

Terminal Number | Wire Colour | Signal | Description | Measuring Conditions/Terminal Voltage
B7 | GRN/WHT | HLC LSP | CVT pulley pressure control valve assembly power supply positive electrode | With ignition switch ON (II): Pulsing signal
B16 | YEL/GRN | SC LSP | CVT start clutch pressure control valve assembly power supply positive electrode | With ignition switch ON (II): Pulsing signal
B24 | BLU/WHT | SH LSP | CVT speed change control valve assembly power supply positive electrode | With ignition switch ON (II): Pulsing signal

PCM CONNECTOR C (22P)

Terminal Number | Wire Colour | Signal | Description | Measuring Conditions/Terminal Voltage
C1 | BLK/RED | HLC LSM | CVT pulley pressure control valve assembly power supply negative electrode |
C6 | GRN/RED | SOL INH | Inhibitor solenoid control | With inhibitor solenoid ON: Battery voltage With inhibitor solenoid OFF: 0 V
C7 | RED/BLU | NDR | CVT drive pulley speed sensor signal input | In other than and position: Pulsing signal
C8 | BLU/RED | SC LSM | CVT start clutch pressure control valve assembly power supply negative electrode |
C9 | RED | ATP S | Transmission range switch position input | In position: 0 V In other than position: 5 V
C10 | WHT | ATP R | Transmission range switch position input | In position: 0 V In other than position: Battery voltage
C11 | BLU | ATP L | Transmission range switch position input | In position: 0 V In other than position: 5 V