## Automatic Transmission

#### A/T Clutch Pressure Control Solenoid Valves A and B Replacement

14-119

Mainshaft Speed Sensor Replacement

1. Remove the mounting bolts and the A/T clutch pressure control solenoid valves A and B.

2. Clean the mounting surface and fluid passage of the A/T clutch pressure control solenoid valves A and B and the transmission housing.
3. Install the new filter/gasket (C) in the solenoid valve assembly body groove.
4. Install the new A/T clutch pressure control solenoid valves A and B. Do not pinch the filter/gasket.
5. Check the A/T clutch pressure control solenoid valve connectors for rust, dirt, or oil, then connect them securely.

1. Disconnect the mainshaft speed sensor connector.

2. Remove the mainshaft speed sensor (A) and sensor washer (B).

   NOTE: The mainshaft speed sensor washer is equipped on the SLXA transmission; the BMXA transmission does not have it.

3. Install the new mainshaft speed sensor with the new O-ring (C) and mainshaft speed sensor washer (SLXA transmission).
4. Check the mainshaft speed sensor connector for rust, dirt, or oil, then connect the connector securely.