## Fuel and Emissions Systems

#### DTC Troubleshooting Index

11-6

DTC | Indicate Lamp | Detection Item | Page
Scan tool DTC | Honda DTC | MIL (Check Engine Lamp) | Glow Lamp |  |
P0101 | - | On | - | MAF System Performance | (see page 11-47)
P0102 | - | On | - | MAF Sensor Circuit Low Voltage | (see page 11-49)
P0103 | - | On | - | MAF Sensor Circuit High Voltage | (see page 11-51)
P0112 | - | On | - | IAT Sensor Circuit Low Voltage | (see page 11-53)
P0113 | - | On | - | IAT Sensor Circuit High Voltage | (see page 11-54)
P0117 | - | On | - | ECT Sensor Circuit Low Voltage | (see page 11-55)
P0118 | - | On | - | ECT Sensor Circuit High Voltage | (see page 11-56)
P0192 | - | On | On | RP Sensor Circuit Low Voltage | (see page 11-57)
P0193 | - | On | On | RP Sensor Circuit High Voltage | (see page 11-59)
P0223 | - | On | On | Accelerator Pedal Position (APP) Sensor 1 Circuit High Voltage | (see page 11-60)
P0228 | - | On | On | Accelerator Pedal Position (APP) Sensor 2 Circuit High Voltage | (see page 11-62)
P0236 | - | On | - | MAP System Performance | (see page 11-63)
P0237 | - | On | - | MAP Sensor Circuit Low Voltage | (see page 11-65)
P0238 | - | On | - | MAP Sensor Circuit High Voltage | (see page 11-66)
P0335 | - | On | On | CKP-CMP Correlation Error | (see page 11-67)
P0338 | - | On | On | Over Speed Detection | (see page 11-69)
P0341 | - | On | On | CMP Sensor Circuit Performance | (see page 11-70)
P0343 | - | On | On | CMP Sensor Signal Too High Frequency | (see page 11-72)
P0501 | - | On | On | Vehicle Speed Sensor (VSS) Signal Too High Frequency | (see page 11-74)
P0502 | - | On | On | VSS Circuit Low Input | (see page 11-75)
P0503 | - | On | On | Vehicle Speed Sensor (VSS) Signal Above Upper Limit | (see page 11-76)
P0562 | - | On | - | System Voltage Low | (see page 11-77)
P0563 | - | On | - | System Voltage High | (see page 11-79)
P0601 | - | On | - | ECM Memory (Checksum Error) | (see page 11-81)
P0606 | - | On | On | Redundant Overrun Monitoring | (see page 11-81)
P0704 | - | On | On | No Clutch SW Signal | (see page 11-82)
P1000 | - | On | On | Injector Low Side Circuit Over Current (Short to Bolt) | (see page 11-83)
P1001 | - | On | On | Injector High Side Circuit Over Current (Short to ground) | (see page 11-85)
P1002 | - | On | On | Injector 1 Low Current Open Circuit | (see page 11-87)
P1003 | - | On | On | Injector Performance Malfunction | (see page 11-88)
P1007 | - | On | On | Injector 2 Low Current Open Circuit | (see page 11-89)
P1012 | - | On | On | Injector 3 Low Current Open Circuit | (see page 11-90)
P1017 | - | On | On | Injector 4 Low Current Open Circuit | (see page 11-91)

a a a