## Cylinder Head

#### Timing Belt Removal (cont'd)

6-19

6. Remove the adjust plate mounting bolt (A), locknut (B) and mounting bolt (C), then remove the power steering (P/S) pump belt (D) and pump without disconnecting the P/S hoses.

7. Remove the alternator (see page 4-32).
8. Remove the four ignition coils (see page 4-24).
9. Remove the throttle cable clamps (A) and harness holder (B) from the cylinder head cover.

10. Remove the cylinder head cover.