## Openers

#### Trunk Lid Opener/Fuel Fill Door Opener Cable Replacement (cont'd)

20-127

5. Remove the cushion tape (A), and detach the clip (B) with a clip remover. Remove the fuel fill door latch (C) by turning it 90°, and detach the opener cable junction box (D) from the body.

   Fastener Locations
   A: Cushion tape, 1 | B and G : Clip, 2 | H: Clip, 3

6. Disconnect the trunk lid opener cable (E) from the trunk lid latch (F) (see page 20-1 30).
7. Using a clip remover, detach the clip (G) from the body, and detach the clips (H) from the trunk lid hinge.
8. Remove the trunk lid opener/fuel fill door opener cable from the vehicle. Take care not to bend the cable.
9. Install the opener cable in the reverse order of removal, and note these items:

- Align the mark on the cable with the clip on the bottom portion of the trunk lid hinge.
- Replace any damaged clips.