## Glass

#### Quarter Glass Replacement (cont'd)

20-189

12. Align the upper clip (A) and lower clip (B) with the front seal (C), then glue them to the inside face of the quarter glass and align the centre of the rear clip (D) with the alignment mark (E) you made in step 10 and glue it to the inside face of the quarter glass as shown. Be careful not to touch the glass where adhesive will be applied.

13. With a sponge, apply a light coat of glass primer along the edge of the glass (A) and seal (B) as shown, then lightly wipe it off with gauze or cheesecloth:

- With the alignment lines (C) on the quarter glass as a guide, apply the glass primer to the upper and lower corner portions of the quarter glass.
- Do not apply body primer to the quarter glass and do not get body and glass primer sponges mixed up.
- Never touch the primed surfaces with your hands. If you do, the adhesive may not bond to the quarter glass properly, causing a leak after the quarter glass is installed.
- Keep water, dust and abrasive materials away from the primed surface.

Hatched area: Apply body primer here