## Cylinder Head

#### Rocker Arm Assembly Removal

6-28

1. Remove the cam chain (see page 6-13).

1. Loosen the rocker arm adjusting screws (A).

1. Remove the camshaft holder bolts. To prevent damaging the camshafts, unscrew the bolts two turns at a time, in a crisscross pattern.

   CAMSHAFT HOLDER BOLTS LOOSENING SEQUENCE:

1. Remove the cam chain guide B, camshaft holders and camshafts.

1. Insert the bolts (A) into the rocker shaft holder, then remove the rocker arm assembly (B).

a a a