## Doors

#### Rear Door Panel Removal/Installation

20-15

Special Tools Required Trim pad remover, Snap-On # A 177 or equivalent, commercially available.

1. If applicable, remove the regulator handle (A) by pulling the clip (B) out with a wire hook (C).

2. Remove the inner handle (A). Take care not to scratch the door panel.

1. Pry out on the upper portion of the cover (B) to release the hooks (C, D), then remove the cover.
2. Remove the screws.
3. Pull out the inner handle forward and out half-way to release the hook (E).
4. Disconnect the inner handle rod (F).

   Fastener Locations
   : Screw, 2

3. Remove the grip cover (A).

1. Using a flat-tip screwdriver wrapped with protective tape, pry out the front edge of the cover to release the clip (B).
2. Pry out along the bottom to release the lower hooks (C).
3. Pry out along the top to release the upper hooks (D), and release the clip (E) while pulling the cover forward.

   Fastener Locations
   C : Hook, 5 | D : Hook, 4 | : Screw, 2

4. Remove the screws from the grip base (F).