## Shafts and Clutches

#### Clutch Inspection (cont'd)

14-209

2ND/4TH CLUTCH

1. O-RING, Replace
2. CLUTCH PISTON
3. RETURN SPRING
4. SPRING RETAINER
5. SNAP RING
6. CLUTCH PLATES, 3

   Standard thickness:

   2.0 mm (0.079 in.)

7. CLUTCH END PLATE
8. SNAP RING
9. CLUTCH DISCS, 3

   Standard thickness:

   1.94 mm (0.076 in)

1. CLUTCH PLATES, 3

   Standard thickness:

   2.0 mm (0.079 in)

2. SNAP RING
3. CLUTCH END PLATES
4. CLUTCH DISCS, 3

   Standard thickness:

   1.94 mm (0.076 in.)

5. SNAP RING
6. SPRING RETAINER
7. RETURN SPRING
8. WAVE SPRING
9. CLUTCH PISTON
10. O-RING, Replace.
11. 4TH CLUTCH DRUM
12. 2ND CLUTCH DRUM