## Exterior Lights

#### Taillight Replacement (cont'd)

22-119
Side Turn Signal Lights Replacement

Taillights (5-door):

1. Remove the rear bumper (see page 20-244).
2. Open the tailgate and disconnect the connectors (A) from the taillight (B).

   Brake/Taillight: | 21/5 W
   Turn Signal Light: | 21 W
   Back-Up Light: | 21 W
   Rear Fog Light: | 21 W (KE model)

3. Turn the bulb socket 45º counter-clockwise to remove the bulb socket.
4. Remove the mounting nuts and bolts, then remove the taillight.
5. When installing the taillight, check for the gasket; if it is distorted or stays compressed, replace it.
6. After installing the taillight, run water over the taillight to make sure they do not leak.

NOTE: Be careful not to damage the fender.

1. Push the retaining spring (A) and remove the side turn signal light (B).

Side Turn Signal Light: 5W

2. Disconnect the 2 P connector (C) from the light.