## Intake Manifold and Exhaust System

#### Exhaust Pipe and Muffler Replacement(cont'd)

9-7

NOTE: Use new gaskets and self-locking nuts when reassembling.

D15Y3, D16V2, D17A5 engines:

1. GASKET

   Replace.

2. MUFFLER
3. 8 x 1.25 mm

   22 Nm (2.2 kgf/m, 16 lbf/ft)

   Replace.

   Tighten the bolts in steps, alternating side-to-side

4. HEATSHIELD
5. EXHAUST PIPE B
6. GASKET

   Replace.

7. EXHAUST PIPE A
8. 8 x 1.25 mm

   22 Nm (2.2 kgf/m, 16 lbf/ft)

   Replace.

   Tighten the bolts in steps, alternating side-to-side

9. GASKET

   Replace.

10. SELF-LOCKING NUT

    10 x 1.25 mm

    33 N (3.4 kgf/m, 25 lbf/ft)

    Replace.