## Manual Transmission

#### Transmission Disassembly (cont'd)

13-16

Exploded View – Transmission Housing

1 | TRANSMISSION HOUSING | 9 | 72 mm SHIM | 18 | 6 mm FLANGE BOLT
2 | 32 mm SEALING CAP |  | (Turkey-produced D14Z6 |  | 12 Nm (1.2 kgf/m, 9 lbf/ft)
| 25 Nm (2.5 kgf/m, 18 lbf/ft) |  | engine transmission) | 19 | BACK-UP LIGHT SWITCH
3 | 35 x 58 x 8 mm OIL SEAL |  | 80 mm SHIM |  | 25 Nm (2.5 kgf/m, 18 lbf/ft)
| Replace |  | (Except Turkey-produced | 20 | 18 mm WASHER
4 | DRAIN PLUG |  | D14Z6 engine transmission) |  | Replace
| 39 Nm (4.0 kgf/m, 29 lbf/ft) | 10 | OIL GUTTER PLATE | 21 | DETENT BOLTS
5 | 14 mm WASHER | 11 | SNAP RING |  | 22 Nm (2.2 kgf/m, 16 lbf/ft)
| Replace | 12 | 72 mm SHIM | 22 | 12 mm WASHER
6 | FILLER PLUG | 13 | OIL GUIDE PLATE M |  | Replace
| 44 Nm (4.5 kgf/m, 33 lbf/ft) | 14 | 8 x 10 mm DOWEL PIN | 23 | SPRING L. 23.6 mm (0.93 in.)
7 | 20 mm WASHER | 15 | SHIFT LEVER ASSEMBLY | 24 | STEEL BALL
| Replace | 16 | SELECT LEVER ASSEMBLY | 25 | TRANSMISSION HANGER
8 | 8 mm FLANGE BOLT | 17 | 8 mm FLANGE BOLT | 26 | 8 mm FLANGE BOLT
| 27 Nm (2.8 kgf/m, 20 lbf/ft) |  | 27 Nm (2.8 kgf/m, 20 lbf/ft) |  | 27 Nm (2.8 kgf/m, 20 lbf/ft)