## Relays

#### Power Relay Test (cont'd)

22-81

Normally-open type B: Check for continuity between the terminals.

- There should be continuity between the No. 1 and No. 3 terminals when power and ground are connected to the No. 2 and No. 4 terminals.
- There should be no continuity between the No. 1 and No. 3 terminals when power is disconnected.

Rear window defogger relay

Blower motor relay

type 1:

type 2: