## Cooling System

#### Water Pump Inspection

10-7
Water Pump Replacement

1. Remove the timing belt (see page 6-18).

2. Turn the water pump pulley counter-clockwise. Check that it turns freely.
3. Check for signs of seal leakage. A small amount of ''weeping'' from the bleed hole (A) is normal.

1. Remove the timing belt (see page 6-18).

2. Remove the water pump (A) by removing four bolts.

3. Inspect and clean the O-ring groove and mating surface with the cylinder block.
4. Install the water pump with a new O-ring (B) in the reverse order of removal.
5. Clean up any spilled engine coolant.