## M/T Differential

#### Differential Thrust Clearance Adjustment (cont'd)

13-65

1. If the clearance is more than the standard, select a new shim from the following table. If the clearance measured in step 5 is within the standard, go to step 9.

   80 mm Shim

| Part Number | Thickness
A | 41441-PL3-B00 | 1.0 mm (0.0394 in.)
B | 41442-PL3-B00 | 1.1 mm (0.0433 in.)
C | 41443-PL3-B00 | 1.2 mm (0.0472 in.)
D | 41444-PL3-B00 | 1.3 mm (0.0512 in.)
E | 41445-PL3-B00 | 1.4 mm (0.0551 in.)
F | 41446-PL3-B00 | 1.5 mm (0.0591 in.)
G | 41447-PL3-B00 | 1.6 mm (0.0630 in.)
H | 41448-PL3-B00 | 1.7 mm (0.0669 in.)
J | 41449-PL3-B00 | 1.8 mm (0.0709 in.)
K | 41450-PL3-B00 | 1.05 mm (0.0413 in.)
L | 41451-PL3-B00 | 1.15 mm (0.0453 in.)
M | 41452-PL3-B00 | 1.25 mm (0.0492 in.)
N | 41453-PL3-B00 | 1.35 mm (0.0531 in.)
P | 41454-PL3-B00 | 1.45 mm (0.0571 in.)
Q | 41455-PL3-B00 | 1.55 mm (0.0610 in.)
R | 41456-PL3-B00 | 1.65 mm (0.0650 in.)
S | 41457-PL3-B00 | 1.75 mm (0.0689 in.)

1. Remove the bolts and transmission housing.

1. Replace the thrust shim selected in step 6, then recheck the clearance.

1. Reinstall the transmission.

a a a