## Cylinder Head

#### Timing Belt Removal (cont'd)

6-8

1. Remove the water pump pulley.

1. Remove the crankshaft damper pulley (A) and lower cover (B).

1. Remove the crankshaft position (CKP) sensor.

1. Before removing the timing belt to inspect timing belt for cracks, worn out timing belt teeth, engine oil or coolant stuck on the timing belt.

1. Loosen the fixing bolt of timing belt tensioner (A) and turn belt tension counter clockwise, then retighten the fixing bolt.

1. Remove the timing belt (B).

a a a