## Maintenance Schedule for Normal Conditions

#### (European Model)

3-4

Listed by Distance/Time

Follow the Normal Conditions Maintenance Schedule if the severe driving conditions specified in the Severe Conditions Maintenance Schedule on 3-6 and 3-7 do not apply.

Service at the indicated distance or time whichever comes first. | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200
miles x 1,000 | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
Replace engine oil | l | l | l | l | l | l | l | l | l | l
Replace engine oil filter | l | l | l | l | l | l | l | l | l | l
Replace air cleaner element |  | l |  | l |  | l |  | l |  | l
Inspect valve clearance |  | l |  | l |  | l |  | l |  | l
Replace fuel filter |  |  |  |  |  | l |  |  |  |
Replace spark plugs |  | l |  | l |  | l |  | l |  | l
Replace timing belt, and inspect water pump | Every 120,000 km (72,000 miles) or 96 months
Inspect and adjust drive belts |  | l |  | l |  | l |  | l |  | l
Inspect idle speed |  |  |  |  |  | l |  |  |  |
Replace engine coolant | 200,000 km (120,000 miles) or 120 months, thereafter every 100,000 km (60,000 miles) or 60 months
Replace transmission fluid | Manual Transmission | Every 120,000 km (72,000 miles) or 96 months
Automatic Transmission | 120,000 km (72,000 miles) or 96 months, thereafter every 80,000 km (48,000 miles) or 48 months
Inspect front and rear brakes | l | l | l | l | l | l | l | l | l | l
Replace brake fluid | Every 36 months
Check parking brake adjustment | l | l |  | l |  | l |  | l |  | l
Replace air conditioning filter | Every 30,000 km (18,000 miles) or 12 months
Check light alignment | l | l | l | l | l | l | l | l | l | l
Test drive (noise, stability, dashboard operation) | l | l | l | l | l | l | l | l | l | l
Visually inspect the following items:
Tie rod ends, steering gearbox and boots | l | l | l | l | l | l | l | l | l | l
Suspension components
Driveshaft boots
Brake hoses and lines (including ABS)
All fluid levels and condition of fluid
Exhaust system
Fuel line and connections
Tyre condition