## Fuel and Emissions Systems

#### System Descriptions (cont'd)

11-23

Vacuum Hose Routing (cont'd)

1. 4WAY
2. VSS
3. ASSEMBLE TO VSV.
4. MUST INSERT TO THE END.
5. VSV
6. ASSEMBLE TO 4WAY.
7. INSERTION LENGTH IS MORE THAN 10mm.
8. CLAMP TO HARNESS; P/P
9. EVRV
10. VSV
11. 4WAY
12. ASSEMBLE TO EVRV.
13. MUST INSERT TO THE END.
14. EVR
15. 3WAY
16. INSERTION LENGTH IS MORE THAN 10mm
17. ASSEMBLE TO 3WAY

No. | Part Name | QTY | Remarks
(1) | JOINT; 4WAY | 1 |
(2) | HOSE; VACUUM, V/PIPE-4WAY | 1 | ø7
(3) | HOSE; VACUUM, TURBO-EVRV | 1 | ø10
(4) | HOSE; VACUUM, 4WAY-EVRV (TURBO) | 1 | ø7-ø8 4WAY-EVRV (TURBO)
(5) | HOSE; VACUUM, 4WAY-EVRV (EGR) | 1 | ø7-ø8 4WAY-EVRV (EGR)
(6) | HOSE; VACUUM, 4WAY-VSV | 1 | ø7-ø8 4WAY-VSV
(9) | JOINT; 3WAY | 1 |
(10) | HOSE; VACUUM, TURBO-3WAY | 1 | ø10
(11) | HOSE; VACUUM, EGR-3WAY | 1 | ø10
(12) | HOSE; VACUUM, 3WAY-A/C | 1 | ø10

a a a