## SRS

#### DTC Troubleshooting - with Side Airbags (cont'd)

23-122

9. Check resistance between the No. 8 and No. 15 terminals of the U2o connector. There should be 0 - 1.0 ohm.

U2o CONNECTOR

Wire side of female terminals

Is the resistance as specified?

YES - Faulty left side impact sensor or SRS unit; replace the left side impact sensor. If the problem is still present, replace the SRS unit.

NO - Open in the floor wire harness; replace the floor wire harness.

DTC 13-4: Faulty Power Supply to the Left Side Impact Sensor (Without OPDS Unit Model)

1. Erase the DTC memory (see page 23-38).
2. Turn the ignition switch ON (II), and check that the SRS indicator light comes on for about 6 seconds and then goes off.

Does the SRS indicator light stay on?

YES - Go to step 3.

NO - Intermittent failure, system is OK at this time. Go to Troubleshooting Intermittent Failures (see page 23-38).

3. Turn the ignition switch OFF. Disconnect the battery negative cable and wait for 3 minutes.
4. Disconnect the SLi and SRi connectors.