## Interior Trim

#### Headliner Removal/Installation

20-68

NOTE:

- When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
- Take care not to bend and scratch the headliner.
- Be careful not to damage the dashboard and other interior trim.

1. Remove these items:

- Front pillar trim, both sides (see page 20-64)
- Centre pillar upper trim, both sides (see page 20-64)
- Rear-view mirror (see page 20-36)
- Ceiling light/spotlights, with sunroof (see page 22-137)
- Spotlights, without sunroof (see page 22-138)
- Ceiling light (see page 22-138)

2. From both sides, remove the caps (A), and remove the self-tapping ET screws, then remove the sunvisor (B) and holder (C).

   Fastener Locations
   : Screw, 4

3. Lower the grab handle, then remove the caps (A). Remove the self-tapping ET screws, then remove the grab handle (B). Remove the remaining grab handles.

   Fastener Locations
   : Screw, 6