## Doors

#### Front and Rear Door Glass Adjustment (cont'd)

20-163

7. Check for water leaks. Run water over the roof and on the sealing area as shown, and note these items:

- Use a 12 mm (1/2 in.) diameter hose (A).
- Adjust the rate of water flow as shown (B).
- Do not use a nozzle.
- Hold the hose about 300 mm (12 in.) away from the door (C).

8. Attach the plastic cover and install the door panel, front door (see page 20-144), rear door (see page 20-152).