## Mirrors

#### Power Mirror Replacement

20-170

1. Lower the door glass fully.

2. Carefully pry out the mirror mount cover (A) by hand in the sequence shown.

   Fastener Location
   : Clip, 1

3. Remove the door panel (see page 20-144).

4. Disconnect the connector (A), and detach the harness clip (B). While holding the mirror (C), remove the nuts, then remove the mirror. Take care not to scratch the door.

Fastener Locations
: Nut, 3

5. Install the mirror in the reverse order of removal and note these items:

- Make sure the connector is plugged in properly.
- Attach the harness clip.