## Cylinder Head

####

6-57

TDC Sensor Replacement

1. Remove the grommet (A) from the upper cover and disconnect the TDC sensor connector (B).

2. Remove the upper cover (C).
3. Remove the TDC sensor from the cylinder head.

4. Install the TDC sensor in reverse order of removal.

CKP Sensor Replacement

1. Remove the grommet (A) from the upper cover and disconnect the TDC sensor connector (B).

2. Remove the upper cover (C) and lower cover (D).
3. Disconnect the CKP sensor connector, then remove the CKP sensor from the oil pump.

4. Install the CKP sensor in reverse order of removal.