## Rear Panel

#### Removal

3-30

- Cut and pry off the rear panel.

NOTE: When removing the rear panel side stiffener attached to the rear combination adaptor, if possible.

- Check the rear combination adaptor position and for damage and if necessary, remove the rear panel side stiffener, and replace the rear combination adaptor and rear gutter as an assembly.

  1. REAR PANEL SIDE STIFFENER
  2. REAR COMBINATION ADAPTOR
  3. REAR PANEL
  4. REAR PANEL GUSSET
  5. REAR PANEL GUSSET
  6. REAR FLOOR
  7. REAR PANEL
  8. REAR PANEL SIDE STIFFENER
  9. REAR COMBINATION ADAPTOR