## Standards and Service Limits

#### Brakes

2-7

Item | Measurement | Qualification | Standard or New | Service Limit
Parking brake lever | Distance travelled when pulled with 196 N (20 kgf, 44 lbs) of force | 3-door | 7 – 8 clicks
5-door | 7 – 8 clicks
Brake pedal | Pedal height (Carpet removed) | 3-door | 184 mm (7.24 in.)
5-door | 180 mm (7.09 in.)
Free play |  | 0.4 – 3.0 mm (0.016 – 0.118 in.)
Master cylinder | Piston-to-pushrod clearance |  | 0 – 0.4 mm (0 – 0.02 in.)
Brake disc | Thickness | Front | 20.9 – 21.8 mm (0.82 – 0.86 in.) | 21.0 mm (0.83 in.)
Rear | 8.9 – 9.1 mm (0.350 – 0.358 in.) | 9.0 mm (0.35 in.)
Runout |  | – | 0.10 mm (0.004 in.)
Parallelism |  | – | 0.015 mm (0.0006 in.)
Brake pads | Thickness Front |  | 10.5 – 11.5 mm (0.41 – 0.45 in.) | 1.6 mm (0.06 in.)
| 9.0 – 10.0 mm (0.35 – 0.39 in.) | 1.6 mm (0.06 in.)
Thickness Rear |  | 9.5 – 10.5 mm (0.37 – 0.41 in.) | 1.6 mm (0.06 in.)
Brake booster Vehicle with ABS | Characteristics at 196 N (20 kgf, 44 lbf) pedal force | Vacuum kPa (mmHg, inHg) | N (kgf, lbf) | kPa (kgf/cm2, psi)
0 (0, 0) | 98 (10, 22) | 0 (0, 0)
294 (30, 66) | 1700 (17, 240)
66.7 (500, 19.7) | 98 (10, 22) | 4600 (47, 670)
294 (30, 66) | 10500 (107, 1500)

Air Conditioning

Item | Measurement | Qualification | Standard or New
Refrigerant | Type |  | HFC-134 a (R-134 a)
Capacity or system |  | 500 – 550 g (17.6 – 19.4 oz)
Refrigerant oil | Type |  | DH-PS
Capacity of components | Condenser | 25 ml (5/6 fl oz, 0.9 lmp oz)
Evaporator | 45 ml (1 1/2 fl oz, 1.3 lmp oz)
Each line and hose | 10 ml (1/3 fl oz, 0.4 lmp oz)
Receiver | 10 ml (1/3 fl oz, 0.4 lmp oz)
Compressor | 140 – 150 ml (4 2/3 fl oz, 4.9 lmp oz – 5 fl oz, 5.2 lmp oz)
Compressor | Clutch coil resistance | at 68°F (20°C) | 3.57 – 3.79 ohms
Pulley-to-pressure plate clearance |  | 0.3 – 0.6 mm (0.01 – 0.02 in.)

a a a