## Cylinder Head

#### Cylinder Head Installation (cont'd)

6-53

17. Install the A/C hose bracket (A) and P/S hose bracket (B).

18. Loosely install the alternator.
19. Adjust the alternator belt tension (see page 4-38) or the alternator-compressor belt tension (see page 4-37).
20. Loosely install the P/S pump belt and pump.
21. Adjust the P/S pump belt (see page 17-23).
22. Install the connecting pipe (A) with a new O-ring (B).

23. Install the ground cable (A), upper radiator hose (B), lower radiator hose (C), heater hose (D) and water bypass hose (E).

24. Install the EVAP canister hose.