## Honda Multi Matic Transmission/CVT

#### Transmission Installation (cont'd)

14-335

25. Install the splash shield.

26. Install the front mount bolt.

27. Remove the hoist and remove the hoisting bracket from the engine.

28. Connect the primary HO2S connector (A) and install the harness (B) on its clamps (C).

29. Connect the ATF cooler hoses (A) to the ATF cooler lines (B) (see page 14-338).