## Interior Trim

#### Trim Removal/Installation - Rear Side Area

20-30

NOTE:

- Put on gloves to protect your hands.
- When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
- Take care not to bend or scratch the trim and panels.

To remove the rear side trim panel, remove these items:

- Rear seat cushion and rear seat-back (see page 20-40)
- Trunk floor mat and spare tyre lid (see page 20-31)
- Trunk side spacers, for some models (see page 20-31)
- Rear trim panel (see page 20-31)

Remove the trim as shown. On the right side, disconnect the trunk compartment light connector.

Install the trim in the reverse order of removal and note these items:

- Replace any damaged clips.
- Make sure the trunk compartment light connector is plugged in properly.
- If the threads on the rear side trim panel mounting self-tapping ET screws are worn out, use an oversized self-tapping ET screw made specifically for this application.
- When installing the rear side shelf, slip the rear seat belt through the slit in the trim.
- Before installing the anchor bolts, make sure there are no twists or kinks in the belt.

Fastener Locations

A : Clip, 11 B : Clip, 1 C : Clip, 1

(White)

1. LID
2. REAR CENTRE SHELF
3. REAR PILLAR TRIM
4. REAR SIDE SHELF
5. REAR SEAT BELT
6. SLIT
7. REAR SIDE TRIM PANEL
8. REAR SEAT STRIKER CAP
9. CENTRE PILLAR UPPER TRIM
10. REAR SPEAKER CONNECTOR
11. DOOR SILL TRIM
12. FRONT SEAT BELT LOWER ANCHOR BOLTS

    7/16-20 UNF

    32 Nm (3.3 kgf/m, 24 lbf/ft)

13. REAR SPEAKER

    (For some models)

14. REAR SPEAKER LID
15. Without trunk side spacers model.
16. REAR BULKHEAD COVER
17. SELF-TAPPING ET SCREWS

    5 x 0.8 mm

    4 Nm (0.4 kgf/m, 3 lbf/ft)

a a a