## Automatic Transmission

#### Transmission Installation (cont'd)

14-133

22. Connect the ball joints (A) to the lower arms (B) and install the castle nuts (C) and spring clips (D).

23. Connect the ball joint pins (E) to the lower arms and install the nuts (F). Insert a 5 mm Allen wrench (G) in the top of the ball joint pins and tighten the nuts.
24. Install the exhaust pipe A.

25. Connect the secondary HO2S connector and install the harness on its clamp.

26. Install the front mount (A). Tighten the mount bolt (B) loosely and tighten the mounting bolts (C) to the specified torque, then tighten the mount bolt to the specified torque.

27. Connect the primary HO2S connector (D) and install it on its bracket (E). Install the harness (F) on its clamp (G).