## A/T Gear Position Indicator

#### Transmission Range Switch Test

14-350

1. Disconnect the transmission range switch connector.

Connector Terminal Description

No. | Description | No. | Description
1 | ATP NP | 6 | Not connected
2 | GND | 7 | Not used
3 |  | 8 |
4 |  | 9 |
5 |  | 10 |

2. Check for continuity between terminals at the switch connector. There should be continuity between terminals below listed for each switch position.

In position, between terminals:

- No. 1 and No. 2
- No. 1 and No. 10
- No. 2 and No. 10

In position, between terminals:

- No. 2 and No. 5

In position, between terminals:

- No. 1 and No. 2
- No. 1 and No. 9
- No. 2 and No. 9

In position, between terminals:

- No. 2 and No. 4

In position, between terminals:

- No. 2 and No. 8

In position, between terminals:

- No. 2 and No. 3
- If there is no continuity between any terminals, adjust the transmission range switch installation. If the transmission range switch installation is OK, replace the transmission range switch.
- If the transmission range switch continuity check was OK, replace the faulty transmission harness.