## Driveline/Axle

#### Driveshafts Installation (cont'd)

16-20

1. Connect the front stabiliser link (A) to the lower arm. Hold the stabiliser link ball joint pin (C) with a hex wrench (D) and tighten the new flange nut (E).

1. Install a new spindle nut (A), then tighten the nut. After tightening, use a drift to stake the spindle nut shoulder (B) against the driveshaft.

1. Clean the mating surfaces of the brake disc and the front wheel, then install the front wheel with the wheel nuts.

1. Refill the transmission with recommended MTF (see page 13-4).

1. Check the front wheel alignment and adjust it if necessary (see page 18-4).

a a a