## Maintenance Schedule for Severe Conditions

#### (European Model)

3-4

Listed by Distance/Time

Service at the indicated distance or time whichever comes first. | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200
miles x 1,000 | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
Replace engine oil | Every 10,000 km (6,000 miles) or 6 months
Replace engine oil filter |  |  |  |  |  |  |  |  |  |
Replace air cleaner element |  |  |  |  |  |  |  |  |  |
Inspect valve clearance | Every 40,000 km (24,000 miles)
Replace fuel filter |  |  |  |  |  |  |  |  |  |
Replace spark plugs | Every 40,000 km (24,000 miles)
Replace timing belt and inspect water pump |  |  |  |  |  |  |  |  |  |
Inspect and adjust drive belts |  |  |  |  |  |  |  |  |  |
Inspect idle speed |  |  |  |  |  |  |  |  |  |
Replace engine coolant | 200,000 km (120,000 miles) or 120 months, thereafter every 100,000 km (60,000 miles) or 60 months
Replace transmission fluid | Manual Transmission | Every 60,000 km (36,000 miles) or 48 months
Automatic Transmission | 60,000 km (36,000 miles) or 48 months, thereafter every 40,000 km (24,000 miles) or 24 months
Inspect front and rear brakes | Every 10,000 km (6,000 miles) or 6 months
Replace brake fluid | Every 36 months
Check parking brake adjustment |  |  |  |  |  |  |  |  |  |
Replace air conditioning filter | Every 30,000 km (18,000 miles) or 12 months
Check light alignment |  |  |  |  |  |  |  |  |  |
Test drive (noise, stability, dashboard operation) |  |  |  |  |  |  |  |  |  |
Visually inspect the following items:
Tie rod ends, steering gearbox and boots | Every 10,000 km (6,000 miles) or 6 months
Suspension components
Driveshaft boots
Brake hoses and lines (including ABS) |  |  |  |  |  |  |  |  |  |
All fluid levels and condition of fluid
Exhaust system
Fuel line and connections
Tyre condition

Follow the Severe Conditions Maintenance Schedule if the customer's vehicle is driven MAINLY under one or more of the following conditions:

- Driving less than 8km (5 miles) per trip or, in freezing temperatures, driving less than 16km (10 miles) per trip.
- Driving in extremely hot over 35°C (95°F) conditions.
- Extensive idling of long periods of stop-and-go driving.
- Trailer towing, driving with a car-top carrier, or driving in mountainous conditions.
- Driving on muddy, dusty, or de-iced roads.

a a a