## Manual Transmission

#### Transmission Disassembly (cont'd)

13-16

Exploded View-Transmission Housing

1 2 3 4 5

6

7

8

9

10

11

12

13

TRANSMISSION REAR COVER

8 x 1.25 mm FLANGE BOLT

19 Nm (1.9 kgf/m,14 lbf/ft)

10 x 1.5 mm FLANGE BOLT

42 Nm (4.3 kgf/m, 31 lbf/ft)

INPUT SHAFT REAR COVER GUTTER

REAR COVER WASHER

6 x 1.0 mm OIL GUTTER BOLT

SLEEVE AND HUB NUT

INSERT STOPPER PLATE

5TH SYNCHRONISER ASSEMBLY

5TH GEAR UNIT

INPUT 5TH GEAR

TRANSMISSION CASE BEARING RETAINER

5TH GEAR THRUST WASHER

8 x 1.25 mm TORX SCREW

26 Nm (2.7 kgf/m, 20 lbf/ft)

14

15

16

17

18

19

20

21

22

23

OUTPUT 5TH GEAR

5TH GEAR NEEDLE BEARING

5TH GEAR NEEDLE BEARING COLLAR

5TH BLOCK RING

8 x 1.25 mm FLANGE BOLT

19 Nm (1.9 kgf/m, 14 lbf/ft)

WASHER

BACK-UP LIGHT SWITCH

39 Nm (4.0 kgf/m, 29 lbf/ft)

CONTROL BOX ASSEMBLY

REAR OUTPUT SHAFT BEARING OUTER RACE AND OUTPUT SHAFT BEARING SHIM

DIFFERENTIAL SIDE BEARING OUTER RACE AND DIFFERENTIAL SIDE BEARING SHIM

24

25

26

27

28

29

30

31

32

10 x 1.5 mm FLANGE BOLT

38 Nm (3.8 kgf/m, 28 lbf/ft)

10 x 1.5 mm BOLT

38 Nm (3.8 kgf/m, 28 lbf/ft)

DRAIN PLUG AND FILLER PLUG

39 Nm (4.0 kgf/m, 29 lbf/ft)

PLUG O-RING

DRIVE SHAFT OIL SEAL

6 x 1.0 mm TRANSMISSION CASE OIL GUTTER BOLT

6 Nm (0.6 kgf/m, 52 lbf/ft)

TRANSMISSION CASE OIL GUTTER

TRANSMISSION CASE

DETENT PLUGS, DETENT SPRING AND DETENT BALLS

25 Nm (2.5 kgf/m, 18 lbf/ft)

TRANSMISSION HANGER

a a a