## Rear Panel

#### Installation

3-31

1. Set the new rear panel and rear combination adaptor into position and clamp them.
   Check the body dimensions (see section 4).

1. NEW REAR COMBINATION ADAPTOR
2. NEW REAR PANEL

1. Tack weld the clamped position.
2. Temporarily install the trunk lid, tailgate, rear bumper and check for difference in level and clearance. Check for operation of the truck lid.
3. Perform the main welding:

- Weld the rear combination adaptor, rear gutter, outer panel and rear panel.

1. OUTER PANEL
2. NEW REAR GUTTER
3. NEW REAR COMBINATION ADAPTOR
4. NEW REAR PANEL

- In the case of leave the rear panel side stiffener and rear combination adopter and replace rear panel.
- Remove the new panel side stiffener from the new rear panel.
- Weld the rear panel side lower stiffener and rear panel side stiffener.

1. REAR COMBINATION ADAPTOR
2. REAR PANEL SIDE STIFFENER
3. REAR PANEL SIDE LOWER STIFFENER

   (New Part)

- Weld the rear panel and rear floor.

1. NEW REAR PANEL